Parameter Description/Value Window material quartz Quantum efficiency at 500 nm 13 % Anode dark current 1 nA Pulse linearity per channel (±2% deviation) 0.5 mA Cross-talk 1 % Uniformity between each anode 1:2.5 Photocasode material bialkali Spectral response 300 ∼ 650 nm Number of stages 12 Anode array of 4 × 4 Pixel size 4 mm ∼ 4 mm Maximum high voltage 1000 V Anode pulse rise time ≤ 1 nsec

Table 1: Characteristics of the Hamamatsu H6568-16MOD photomultiplier, as specified for the Miniplug Calorimeter.